Fire District 13 (Station 55/58/13) Probationary FF Study Sheet

DOT HazMat Books Locations (In Truck)
	Engine 55,58, Tanker 58, Rescue 58 – Glove Box under computer.
	Engine 258 – Center Console
MSDS/SDS Sheets Locations 
Station 55 – Downstairs Computer Desk Drawer (Eye Wash Station in Bay near rear exit door.)
Station 58 – Day Room Computer Desk Drawer (Eye Wash Station in Washer Room in shower)
	Station 13 – Inside the Podium in Training room
Station Phone Numbers
	Station 55 – (336) 621-1551
	Station 58 – (336) 644-9060
Station 13 – (336) 375-5507 (Call this number at a decent hour if you’re calling in Sick or wanting to take a Call Back.  This is where the OIC will be located)
Station Addresses
	Station 55 – 4629 Hicone Rd. Greensboro, NC-27405
	Station 58 – 6912 Spencer Dixon Rd. Greensboro, NC-27455
	Station 13 – 2505 Lees Chapel Rd. Greensboro, NC-27405
Fire District 13 Apparatus
Engine 55 & 58 (Pump – 1500GPM, Tank Capacity – 1000 Gal)
Tanker 58 (Pump – 1250GPM, Tank Capacity – 1800 Gal) (3 Sides Newton/Gravity Dump)
Engine 258 (Pump – 1250 GPM, Tank Capacity – 1500 Gal)
Rescue 58


Fire District 13 Apparatus Cont.

Ladder Lengths and Count
Engine 58,55 (24’ extension, 14’ roof, 10’ Attic/Folding, 2’ “Kallam” Stepladder)
	# of Ladders - 4
	Tanker 58 (35’ Extension, 14’ Roof, 10’ Attic/Folding Ladder)
		# of Ladders - 3
	Rescue 58 (24’ Extension, 14’ Roof, 10’ Attic/Folding, Little Giant Ladder)
		# of Ladders - 4
	Engine 258 (35’ Extension, 14’ Roof, 10’ Attic/Folding Ladder)
		# of Ladders – 3

Apparatus Hose (Pre-Connected Length and Nozzles, Total Amount of Hose on Truck)
	Engine 55,58 -  
2 – 200’ 1 ¾” Crosslays, Packed as Modified Minute-Man Load. (Pre-Connected)
		RED - Left Crosslay (Comes off Drivers-Side) Smoothbore Nozzle (145PSI/150GPM)
		YELLOW - Right Crosslay (Comes of Captain-Side) Fog Nozzle (145PSI/150GPM)
	Front Bumper (Pre-Connected)
		ORANGE - 1 – 100’ 1 ¾”, Single Stack Modified Load W/ Fog Nozzle(110PSI/150GPM)
		1 – 200’ 2 ½” W/ Blitz Nozzle (200PSI/500GPM) (Ground Masterstream)
	Rear-Top 
		GREEN - Pre-Connect – 1 – 200’ 2 ½” W/Smoothbore (76PSI/250GPM)
		Apartment Lay (Not Preconnected) 300’ 2 ½” with Gated Y 
		LDH – 1000’ of 4” (Not Preconnected)
	Engineers Side Middle Compartment
BLUE – Bundle (Highrise Pack) 1 – 100’ 1 ¾” W/ Smoothbore Nozzle (Modified Pack w/ Straps)
	Engineers Pump Panel
		25’ of 4” Double Donut
		“Filler Hose/Nursing Line” - 50’ of 3” Double Donut
	Passengers-Side Pump Panel
		50’ of 4” Connected to Master Steamer Intake
	Engineers Compartment
		2 – 50’ Sections of 1 ¾” hose (Spare)
Total Hose E55/E58
	1 ¾” – 700’
	2 ½” – 700’
	3” – 50’
	4” – 1075’
Tanker 58
2 - 200’ 1 ¾” Crosslays, Packed as Modified Minute-Man Load. (Pre-Connected)
	ORANGE - Left Crosslay (Comes off Drivers-Side) Smoothbore Nozzle (145PSI/150GPM)
	RED – Right Crosslay (Comes off Captains-Side) Fog Nozzle (145PSI/150GPM)
Rear-Top
GREEN - 1 – 200’ 2 ½” (Pre-Connected) Smoothebore Nozzle (76PSI/250GPM)
		LDH - 1000’ of 4” (Not Pre-Connected)
	Passenger-Side Pump Panel
		1 – 50’ of 3” “Nurse Line”
		1 – 25’ of 4”
	Engineers-Side Rear Compartment
		2 – 50’ of 3” W/ Gate-Valve
Total Hose 
	1 ¾” – 400’
	2 ½” – 200’
	3” – 150’
	4” – 1025’
MAIN ROADS 
	Station 55 (Going Down Hicone Rd. Starting w/ Summit Ave)
		Summit Ave.
US-29
		Dunstan Rd.
		McKnight Mill Rd.
		Rankin Mill Rd.
		Eckerson Rd.
		Hines Chapel Rd.
		MCleansville Rd.
	Station 58
		N. Church St.
		Spencer-Dixon Rd
		HWY 150
		Cedar Hollow Rd.
		Air Habor Rd.
		Archergate Rd.
		Yanceyville Rd.
		
Gas Powered Equipment
	Engine 55/58 
		Mixed Gas Equipment
		1 - Regular Chainsaw 
		1 – Carbide Tip Chainsaw (Vent saw)
		1 – K-12 Saw
		Regular Gas Equipment
		1 – Generator 
	

Tanker 58
		Mixed Gas Equipment 
		1 – Regular Chainsaw
		Regular Gas Equipment
		1 – PPV Fan
Rescue 58
		Mixed Gas Equipment
		1 – Regular Chainsaw
		1 – Carbide Tip Chainsaw (Vent Saw) 
		1 – K12
		Regular Gas Equipment
		1 - Portable Holmatro Unit
Engine 258
		Mixed Gas Equipment
		1 – Regular Chainsaw
		1 – Carbide Tip Chainsaw (Vent Saw)
		Regular Gas Equipment
		1 – PPV Fan
		1 – Small Portable Holmatro Unit

Station Duties 58/55
		Sunday – Charge CO/Gas Meters
		Monday – Squad 258 and Engine 258 Weekly Check-Off
		Tuesday – Tankers Weekly Check-Off 
			Training Station 13 @ 9AM
		Wednesday – Engines Weekly Check-Off 
			Training Station 13 @ 9AM
		Thursday – Rescue Weekly Check-Off
			Training Station 13 @ 7PM
Classes of Fire
1. Class A: Solid materials such as wood or paper, fabric, and some plastics
2. Class B: Liquids or Gas such as alcohol, ether, gasoline, or grease
3. Class C: Energized Electrical failure from appliances, electronic equipment, and wiring.
4. Class D: Metal/Metallic substances such as sodium, titanium, zirconium, or magnesium
5. Class K: Grease or oil fires specifically from cooking

Types of Extinguishers at Fire District 13
1. Water-Can (2.5 Gallons in a Pressurized Can) (Class A)
2. ABC (Sodium Bicarbonate) (Class A, B, and C Fires)
3. CO2 (Some Small Class A, and Class C Fires)
Stages of Fire 
1. Incipient
2. Growth 
3. Fully Developed 
4. Decay


When should you obtain your Class B Driver’s License?  *ASAP Before your 6-Month Test.*
What time are we required to be at work and ready for Duty?  0730 is shift start time, on time and ready requires a firefighter to be there at a minimum 15-30 minutes early.
When are timesheets due and who do you send them to?  At a minimum your last shift working before pay period ends (Bi-Weekly) (Friday/Saturday/Sunday) You send them to your OIC.
When do you refill an SCBA bottle on the Trucks?  Below 4000
What type of SCBA do we use at FD13?  MSA 
Where are the Gas Meters Located on Engine 55? Engineers-Side Rear Compartment (Black Pelican Case Box)
How many Airpacks are on each truck?  Rescue 58 – 4, Engine 55 – 8, Engine 58 – 8, Tanker 58 – 4, Engine 258 – 4
Where are the RIT Packs located on the Engines?  Captains-Side Engineers Compartment.
Where is the Cribbing Located on Engine 55 and Engine 58? Rear of Truck Roll-up Door
When backing an Emergency Vehicle always have a backer! (FD13 Policy)
What Daily and Weekly Check Sheets are the FF’s Duty/Responsibility?  Medical Bag & SCBA Check Sheets
When should you check your airpack to make sure its ready for use?  Before YOUR Shift Starts (Before 0730)
What system or website do we use for staff scheduling?  Fire Roster (www.fireroster.com) Login using your FD Provided Email!
When do you check Fire Roster for updates on staffing? When you’re getting off to make sure you don’t need to take your stuff with you and the morning of your shift before leaving your house to make sure you’re going to the right station.
When requesting time-off, what is the process?  Login to Fire Roster select the day you’d like and request leave, sending/adding your OIC to a notification and sending an email to confirm you’ve sent the request.
Where is the Water Can Located on Engine 55 and 58?  Captains side Engineers Compartment (Should be emptied and refilled during first weekly check (Once a Month or as needed, Wednesday’s)
What type of PPV Fans are on the Engines and where are they located?  Electric BlowHard Fans (Approx 20 minutes of usage before needing to be plugged in).  They are located in the captains-side Engineers compartment.
What type of medications do we carry in our Med Bags?  Narcan (Overdoses), Aspirin (Chest pain), Benadryl (Allergic Reactions), Albuterol (With prescription, Asthma or other breathing disorders), Oral Glucose (Low Blood Sugar), Acetaminophen (Fever, and Pain Relief), Epi Jr and Epi Adult (Severe Allergic Reactions)
What day do we clean out the refrigerators at the Station?  Every Sunday!
What day do we clean the mattress covers on all the beds?  Every Sunday or as needed!
What minimum vitals should we take on all medical calls?  Blood Pressure, O2 Stats, Pulse, Breathing Rate, Blood Sugar, Skin Color
[bookmark: _Hlk132056589]What size Winch do we carry on the Trucks?  9000lbs Warn Winch w/ 100’ Cable
Where can the winch be hooked up on the Engines?  Right/Left Rear and Rear of Apparatus 
How many People are assigned to a shift?  7 (Station 55 – 3 (Captain, Engineer, and a Firefighter), Station 58 – 3 (Engineer and 2 Firefighters), Station 13 – 1 (AC))
Who is the Fire Chief? Kevin King
Who are the 8-5 Monday thru Friday Staff?  (AC55 – Donald Jarvis(13), Chief 13 Kevin King(13), Jesse Cottrell(58)
Where are the Bullet Proof Vests located on the Engines? Compartment Under the backseats
What are 5 FF/Rescue Knots you need to know? Bowline, Overhand, Figure 8, Clove Hitch, Figure 8 on a bite
Where is the Vent saw located on the Engines?  Captains side Rear Compartment
Where is the K12 Located on the Engines? Captains side Rear Compartment
Where is the Floating Dock Strainer on the Engines?  Top Compartment Behind Dunnage
Have you downloaded the CalTopo App?  This is for Trail Rescues, Ask Officer!
Where is the Generator located on the Engines? Rear Rollup compartment. E58 &E55
When do we wear our Turnout gear on calls? IDLH Environments (CO/Gas/Fire, Vehicle accidents w/ traffic Vest, or as directed by OIC
Who is the Training Officer?  Jesse Cottrell Stationed at 58 and reachable 8-5 at 336-644-9060 
When do the Trucks get washed?  As needed or on the Weekly Check Day of that apparatus.
When is the Morning Radio Test and what channels do we use for it?  FD13 Private TAC and FD13NEFD Shared Tac, Radio test starts promptly at 0800 unless otherwise on a call or delayed by OIC.













	

