Fire District 13, Inc.

Driver Operator Annual Performance Evaluation Criteria 

PURPOSE

These criteria have been developed to insure that FD13 Driver/Operations are current in the needed knowledge and abilities to perform their duties as Driver/Operators to standards expected by Fire District 13, Inc.  Personnel not passing the process will be allowed to re-test on those sections failed approximately one month after the initial process. 

PREVENTIVE MAINTENANCE
Scope:

The FD13 Driver Operator shall perform routine tests, inspections, and servicing functions on the systems and components specified in the following list, given a fire department vehicle and its manufacturer’s specifications, so that the operational status of the vehicle is verified:

(1)      Battery (ies) 

(2)      Braking system 

(3)      Coolant system 

(4)      Electrical system 

(5)      Fuel 

(6)      Hydraulic fluids 

(7)      Oil 

(8)      Tires 

(9)      Steering system 

(10)    Belts 

(11)    Tools, appliances, and equipment  

Passing Score:
100%

EQUIPMENT LOCATION

Scope:

The FD13 Driver Operator will be tested on his/her knowledge of the location of equipment on each FD13 apparatus by locating the assigned equipment on the assigned apparatus within two minutes.

Passing Score

90%
Process:
1. The FD13 Driver Operator will be given a list of specified equipment for the apparatus they are being evaluated on.
2. The FD13 Driver Operator shall then locate the equipment on the given apparatus, retrieve it, and give a brief description of the function of the tool.

3. Process must be completed within the given time for each apparatus.

4. After equipment is assembled the FD13 Driver Operator shall explain the function of the equipment.

PUMP OPERATIONS

Scope:

The FD13 Driver Operator will be evaluated on his/her ability to perform given pump operation scenarios on various FD13 apparatus.

Passing Score:

100% of objectives

Process:

1. The FD13 Driver Operator will be given a list of directives to demonstrate the knowledge to perform specific task associated with our operations.

2. The FD 13 Driver Operator will perform the following drills utilizing given FD13 apparatus:

#1-Forward lay from a hydrant

#2-Drafting from a portable water supply

#3-Pump the attack pumper with a direct feed tanker

#4-Pump the tanker in a Tanker to Pumper operation

#5-Operate the tanker in a quick dump operation

3. The FD13 Driver Operator shall demonstrate knowledge of the steps of pump operations during all evolutions without compromising water flow.
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